**Manufacturer: Jacksons Fencing**

**Web: www.jacksons-security.co.uk**

**Tel: +44 (0)1233 750393 | 0800 953 3699**

**Product Reference: JAKOUSTIC® COMMERCIAL AND HIGHWAY**

**Service Life of Fencing**

Timber and Steel fencing and gates designed and manufactured to be fit for purpose and providing a minimum 25 year guarantee, delivering the lowest whole life cost and significantly reduced carbon footprint.

**Fencing & Posts:**

Galvanised steel I-beam posts set at 2410mm centres, height above ground required \_\_\_\_\_\_ mm

**Construction:**

Jakoustic® interlocking ‘V’ boards are affixed to galvanised steel I-beam posts for additional strength and rigidity, meeting not only stringent Highways Agency standards BS EN1794-1 and 2, but also ideally suited for application in exposed locations subject to high wind loading. The system is available with matching capping, counter rails and timber cladding to posts to further enhance its appearance. The complete acoustic barri

**Boards:**

Jakcure pressure treated 34mm x 143mm x 4.8m (planed) boards with unique deep interlocking “V” tongue and groove joint

**Posts:**

Galvanised steel 'I' beam posts

Overlength steel I-beam posts

Base plated galvanised steel I-beam posts to bolt down to concrete base foundations

*\* Delete above post options as required*

**Finish / Colour:**

Jakcure® treated timber as standard

Planed timber finish

**Installation**

In accordance to manufacturers instructions

NOTES:

For more information please contact Jacksons Fencing. We reserve the right to alter specification within this document at any time.