**Hit & Miss Panel - Vertical**

Manufacturer: Jacksons Fencing.

Web: www.jacksons-fencing.co.uk.

Tel: +44 (0)1233 750393.

**Product reference:**

Hit & Miss Panel - Vertical

**Width – As Standard:**

1.83m

**Height:**

0.91m

1.22m

1.52m

1.83m

Framing: 45 x 51mm.

Panel Thickness: 51mm

**Gravel Boards:**

Gravel boards are required where panels are in contact with the ground. 140mm added to the height.

**Posts:**

Slotted Jakposts®

**Guarantee:**

All timber used throughout is superior quality Jakcure® treated softwood guaranteed for 25 years.

**Features:**

* All fixings are stainless steel.
* Gravel boards are required where panels are in contact with the ground.
* Panels have a morticed and tenoned frame for extra strength.
* Hit and Miss panels’ design allows some wind and light to pass through. It also allows visibility through the fence at an angle.
* All timber is planed all round.

**Gates:**

Gates are Jakcure® treated softwood, right and left hand hanging (when viewed from the outside) as standard designed to match our Hit & Miss Panel - Vertical.

Height: 1.78m to 1.93m (with capping).

Width: 1m

**Installation**

In accordance to manufacturer’s instructions.

Hit and Miss panels are so called because the boards are alternately fixed on the front and the back of the panel with an over-lap to create a stylish Hit and Miss pattern. They are part of our premium ‘good-both-sides’ range so that both you and your neighbour have the best looking side of the fence, as both sides are the same.

For additional information, please contact Jacksons Fencing. All information within was correct at time of creation. We reserve the right to alter specification without notice.