**Manufacturer: Jacksons Fencing**

**Web: www.jacksons-security.co.uk**

**Tel: +44 (0)1233 750393 | 0800 953 3699**

**Product Reference: 12K ENVIROFENCE®**

**Service Life of Fencing**

Timber fencing and gates designed and manufactured to be fit for purpose and providing a minimum 25 year guarantee, delivering the lowest whole life cost and significantly reduced carbon footprint.

**Fencing & Posts:**

2000mm High, Post Length 2900mm (2410mm Post Centres)

2500mm High, Post Length 3400mm with 2000mm Spur Post (2410mm Post Centres)

3000mm High, Post Length 3900mm with 2500mm Spur Post (2410mm Post Centres)

*\* Delete above as required*

**Boards:**

Jakcure® pressure treated 20mm x 139mm x 4.8m (planed) board with small chamfers which form a V-join between boards. Achieves the planning / architects’ minimum acoustic specification of 10 - 12kg per sqm

**Posts:**

Overlength timber tuning fork posts for setting in concrete as standard

**Fixings:**

Special fixings clamp the acoustic boards between posts

**Finish / Colour:**

Jakcure® treated timber as standard

Planed timber finish

**Installation**

In accordance to manufacturers instructions

NOTES:

For more information please contact Jacksons Fencing. We reserve the right to alter specification within this document at any time.