**Shadowline Panel**

Manufacturer: Jacksons Fencing.

Web: www.jacksons-fencing.co.uk.

Tel: +44 (0)1233 750393.

**Product reference:**

Shadowline Panel

**Width – As Standard:**

1.83m

**Height:**

0.66m

0.91m

Rails: 4 qty 70mm x 24mm back rails.

Thickness: 50mm

Pales: 144x26mm 'Z' board with 110mm raised section and approx 17mm gap, 17mm overlap.

**Gravel Boards:**

Gravel boards are required where panels are in contact with the ground. 140mm added to the height.

**Posts:**

Slotted Jakposts®

**Guarantee:**

All timber used throughout is superior quality Jakcure® treated softwood guaranteed for 25 years.

**Features:**

* All fixings are stainless steel.
* Gravel boards are required where panels are in contact with the ground.
* Panels are stacked to give extra height. (Eg. Two 0.91m panels on top of each other to create a 1.80m approx high panel).
* Offers a modern and contemporary clad design using unique 'Z' boards.
* All fixings are through the back of the panel making the front free of any visible fixings.

**Gates:**

Please speak to our sales team regarding matching gates, which will be made to order.

Height: N/A

Width: Maximum - 1m

**Installation**

In accordance to manufacturer’s instructions.

Built with architectural cladding in mind, our Shadowline Panel has a modern unique profile which provides a dynamic central shadow gap between each board, free of any visible fixings, to provide a seamless contemporary finish. These contemporary panels offer you the option to install a solid privacy style fence with no lines of sight through the panel which creates a clear shadow line between each board.

For additional information, please contact Jacksons Fencing. All information within was correct at time of creation. We reserve the right to alter specification without notice.